MATERIAL INFORMATION

Page 4:1

MATERIAL/INDEX

INDEX	1.50
MATERIAL	CR-39
ABBE	59
DENSITY	1.32
UV BLOCK	96%

Advantages: - Low cost material - Easy to tint - Easy to edge - Stable coating - High abbe value

Disadvantages: - Not recommended for thread or rimless frames - Low index

INDEX	1.60
MATERIAL	MR-8
ABBE	42
DENSITY	1.30
UV BLOCK	100%

Advantages: - very strong material. Recommended for thread or rimless frames - ≈ 20% thinner lens than 1.50 index* - Possible to tint - Stable coating

Disadvantages: - Not possible to tint darker sun colours - Not all Filter colours could be tinted.

INDEX	1.67
MATERIAL	MR-10
ABBE	32
DENSITY	1.35
UV	100%

Advantages: - strong material. Recommended for thread or rimless frames - slightly thinner than 1.60 (≈ 5%)

Disadvantages: - Not possible to tint the material itself (Only by tinting a softer Hard-lacquer) - Low abbe value - Little reduction of thickness compered to 1.60 index (≈ 5%).

INDEX	1.74
MATERIAL	MR-174
ABBE	33
DENSITY	1.47
UV	100%

Advantages: - ≈ 20% thinner lens than 1.60 index* - strong material. Recommended for thread or rimless frames

Disadvantages: - Not possible to tint the material itself (Only by tinting a softer Hard-lacquer) - Low abbe value

Myosoft

* Compered with –8, 65Ømm.

Page 4:2

COATING

ML Prima+
Using the very latest in Coating technology, where all parameters have been upgraded. Increased transmission, more than 35% improved scratch resistance, an antistatic layer which significantly reduces dust and spots and finally the satin layer that gives the lens such a slippery surface (more than 10 times untreated) that it will be cleaned with just one stroke with the cloth.
ML Prima
Our well known basic treatment. A very good multicoat including the upgraded ML Dura, high transmission and the top layer Aqua-coat that reduces the effect of dust
and water.
ML Prima Sun
A treatment designed for sunglasses. Both front and back surface have the ML Dura treatment for increased protection against tear and wear. The back side has the
ML Prima (Prima+ on higher indexes) treatment to increase the comfort and to reduce the annoying reflexes on the inside of dark sunglasses.
ML Dura
Our hard lacquer for improved scratch resistance and optical quality. Now improved with more than 35%. Both sides of the lens are always treated.

Page 4:3

POL 1 Grey

POL 3 Grey

POL Green (G15)

POL Brown

INDEX
Transmission
Polarization

1.50

65%
99%

1.50	1.60	1.67

85%
99%

1.50

85%
99%

1.50	1.60	1.67

81%
99%

Grey

Brown

Brown

INDEX
Transmission
Polarization

1.50	1.60	1.67

3%-85%
-

1.50	1.60	1.67

3%-85%
-

1.50

68%-85%
95%

DIAMETER CHART

INDEX	1.50	1.60	1.67

INDEX	1.50

Page 4:4

Version 2.1